## EmpathyTpCall

EmpathyTpCall

## Synopsis

                        EmpathyTpCall;
    enum                EmpathyTpCallStatus;
    EmpathyTpCall *     empathy_tp_call_new                 (TpChannel *channel);
    void                empathy_tp_call_close               (EmpathyTpCall *call);
    void                empathy_tp_call_to                  (EmpathyTpCall *call,
                                                             EmpathyContact *contact);
    void                empathy_tp_call_accept_incoming_call
                                                            (EmpathyTpCall *call);
    void                empathy_tp_call_request_video_stream_direction
                                                            (EmpathyTpCall *call,
                                                             gboolean is_sending);
    void                empathy_tp_call_start_tone          (EmpathyTpCall *call,
                                                             TpDTMFEvent event);
    void                empathy_tp_call_stop_tone           (EmpathyTpCall *call);
    gboolean            empathy_tp_call_has_dtmf            (EmpathyTpCall *call);

## Object Hierarchy

      GObject
       +----EmpathyTpCall

## Properties

      "audio-stream"             gpointer              : Read
      "channel"                  TpChannel*            : Read / Write / Construct Only
      "contact"                  EmpathyContact*       : Read
      "is-incoming"              gboolean              : Read
      "status"                   guint                 : Read
      "video-stream"             gpointer              : Read

## Description

## Details

### EmpathyTpCall

    typedef struct _EmpathyTpCall EmpathyTpCall;

### enum EmpathyTpCallStatus

    typedef enum
    {
      EMPATHY_TP_CALL_STATUS_READYING,
      EMPATHY_TP_CALL_STATUS_PENDING,
      EMPATHY_TP_CALL_STATUS_ACCEPTED,
      EMPATHY_TP_CALL_STATUS_CLOSED
    } EmpathyTpCallStatus;

### empathy_tp_call_new ()

    EmpathyTpCall *     empathy_tp_call_new                 (TpChannel *channel);

`channel` : |
Returns : |

### empathy_tp_call_close ()

    void                empathy_tp_call_close               (EmpathyTpCall *call);

`call` : |

### empathy_tp_call_to ()

    void                empathy_tp_call_to                  (EmpathyTpCall *call,
                                                             EmpathyContact *contact);

`call` : |
`contact` : |

### empathy_tp_call_accept_incoming_call ()

    void                empathy_tp_call_accept_incoming_call
                                                            (EmpathyTpCall *call);

`call` : |

### empathy_tp_call_request_video_stream_direction ()

    void                empathy_tp_call_request_video_stream_direction
                                                            (EmpathyTpCall *call,
                                                             gboolean is_sending);

`call` : |
`is_sending` : |

### empathy_tp_call_start_tone ()

    void                empathy_tp_call_start_tone          (EmpathyTpCall *call,
                                                             TpDTMFEvent event);

`call` : |
`event` : |

### empathy_tp_call_stop_tone ()

    void                empathy_tp_call_stop_tone           (EmpathyTpCall *call);

`call` : |

### empathy_tp_call_has_dtmf ()

    gboolean            empathy_tp_call_has_dtmf            (EmpathyTpCall *call);

`call` : |
Returns : |

## Property Details

### The `"audio-stream"` property

      "audio-stream"             gpointer              : Read

Audio stream data.

### The `"channel"` property

      "channel"                  TpChannel*            : Read / Write / Construct Only

channel.

### The `"contact"` property

      "contact"                  EmpathyContact*       : Read

Call contact.

### The `"is-incoming"` property

      "is-incoming"              gboolean              : Read

Is media stream incoming.

Default value: FALSE

### The `"status"` property

      "status"                   guint                 : Read

Call status.

Allowed values: <= 255

Default value: 0

### The `"video-stream"` property

      "video-stream"             gpointer              : Read

Video stream data.