## Pentax Tags

The Pentax tags are also used in Asahi cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | PentaxVersion | int8u[4] |
> 0x0001 | PentaxModelType | int16u |
> 0x0002 | PreviewImageSize | int16u[2]~ |
> 0x0003 | PreviewImageLength | int32u* |
> 0x0004 | PreviewImageStart | int32u* |
> 0x0005 | PentaxModelID | int32u | --> Pentax PentaxModelID Values
> 0x0006 | Date | undef[4] |
> 0x0007 | Time | undef[3] |
> 0x0008 | Quality | int16u | 0 = Good 1 = Better 2 = Best 3 = TIFF 4 = RAW

> 0x0009

> PentaxImageSize

> int16u

> 0 = 640x480
> 1 = Full
> 2 = 1024x768
> 3 = 1280x960
> 4 = 1600x1200
> 5 = 2048x1536
> 8 = 2560x1920 or 2304x1728
> 9 = 3072x2304
> 10 = 3264x2448
> 19 = 320x240
> 20 = 2288x1712
> 21 = 2592x1944
> 22 = 2304x1728 or 2592x1944
> 23 = 3056x2296
> 25 = 2816x2212 or 2816x2112
> 27 = 3648x2736
> '0 0' = 2304x1728
> '4 0' = 1600x1200
> '5 0' = 2048x1536
> '8 0' = 2560x1920
> '32 2' = 960x640
> '33 2' = 1152x768
> '34 2' = 1536x1024
> '35 1' = 2400x1600
> '36 0' = 3008x2008 or 3040x2024
> '37 0' = 3008x2000

> 0x000b

> PictureMode

> int16u

> 0 = Program
> 2 = Program AE
> 3 = Manual
> 5 = Portrait
> 6 = Landscape
> 8 = Sport
> 9 = Night Scene
> 11 = Soft
> 12 = Surf & Snow
> 13 = Sunset or Candlelight
> 14 = Autumn
> 15 = Macro
> 17 = Fireworks
> 18 = Text
> 19 = Panorama
> 30 = Self Portrait
> 31 = Illustrations
> 33 = Digital Filter
> 37 = Museum
> 38 = Food
> 40 = Green Mode
> 49 = Light Pet
> 50 = Dark Pet
> 51 = Medium Pet
> 53 = Underwater
> 54 = Candlelight
> 55 = Natural Skin Tone
> 56 = Synchro Sound Record
> 58 = Frame Composite
> '0 0' = Auto
> '0 2' = Program AE
> '5 2' = Portrait
> '6 2' = Landscape
> '9 1' = Night Scene
> '13 1' = Candlelight
> '15 1' = Macro
> '255 0' = Digital Filter?

> 0x000c | FlashMode | N | 0x0 = Auto, Did not fire 0x1 = Off 0x3 = Auto, Did not fire, Red-eye reduction 0x100 = Auto, Fired 0x102 = On 0x103 = Auto, Fired, Red-eye reduction 0x104 = On, Red-eye reduction 0x105 = On, Wireless 0x108 = On, Soft 0x109 = On, Slow-sync 0x10a = On, Slow-sync, Red-eye reduction 0x10b = On, Trailing-curtain Sync
> 0x000d | FocusMode | int16u | (Pentax models) 0 = Normal 1 = Macro 2 = Infinity 3 = Manual 5 = Pan Focus 16 = AF-S 17 = AF-C (Asahi models) 0 = Normal 1 = Macro (1) 2 = Macro (2) 3 = Infinity
> 0x000e | AFPointSelected | int16u | 1 = Upper-left 2 = Top 3 = Upper-right 4 = Left 5 = Mid-left 6 = Center 7 = Mid-right 8 = Right 9 = Lower-left 10 = Bottom 11 = Lower-right 65534 = Fixed Center 65535 = Auto
> 0x000f | AFPointsInFocus | int16u | 0x0 = Fixed Center or Multiple 0x1 = Top-left 0x2 = Top-center 0x3 = Top-right 0x4 = Left 0x5 = Center 0x6 = Right 0x7 = Bottom-left 0x8 = Bottom-center 0x9 = Bottom-right 0xffff = None
> 0x0010 | FocusPosition | int16u | (related to focus distance but affected by focal length)
> 0x0012 | ExposureTime | int32u |
> 0x0013 | FNumber | int16u |
> 0x0014 | ISO | int16u | 3 = 50 4 = 64 5 = 80 6 = 100 7 = 125 8 = 160 9 = 200 10 = 250 11 = 320 12 = 400 13 = 500 14 = 640 15 = 800 16 = 1000 17 = 1250 18 = 1600 21 = 3200 50 = 50 100 = 100 200 = 200 400 = 400 800 = 800 1600 = 1600 3200 = 3200
> 0x0016 | ExposureCompensation | int16u |
> 0x0017 | MeteringMode | int16u | 0 = Multi Segment 1 = Center Weighted 2 = Spot
> 0x0018 | AutoBracketing | int16u[n] | (one or two numbers: exposure bracket step in EV, then extended bracket if available. Extended bracket values are printed as 'WB-BA', 'WB-GM', 'Saturation', 'Sharpness' or 'Contrast' followed by '+1', '+2' or '+3' for step size)
> 0x0019 | WhiteBalance | int16u | 0 = Auto 1 = Daylight 2 = Shade 3 = Fluorescent 4 = Tungsten 5 = Manual 6 = DaylightFluorescent 7 = DaywhiteFluorescent 8 = WhiteFluorescent 9 = Flash 10 = Cloudy 65534 = Unknown 65535 = User Selected
> 0x001a | WhiteBalanceMode | int16u | 1 = Auto (Daylight) 2 = Auto (Shade) 3 = Auto (Flash) 4 = Auto (Tungsten) 7 = Auto (DaywhiteFluorescent) 8 = Auto (WhiteFluorescent) 10 = Auto (Cloudy) 65534 = Preset (Fireworks?) 65535 = User-Selected
> 0x001b | BlueBalance | int16u |
> 0x001c | RedBalance | int16u |
> 0x001d | FocalLength | int32u |
> 0x001e | DigitalZoom | int16u |
> 0x001f | Saturation | int16u | 0 = Low 1 = Normal 2 = High 3 = Med Low 4 = Med High 5 = Very Low 6 = Very High '0 0' = Low '1 0' = Normal '2 0' = High
> 0x0020 | Contrast | int16u | 0 = Low 1 = Normal 2 = High 3 = Med Low 4 = Med High 5 = Very Low 6 = Very High '0 0' = Low '1 0' = Normal '2 0' = High
> 0x0021 | Sharpness | int16u | 0 = Soft 1 = Normal 2 = Hard 3 = Med Soft 4 = Med Hard 5 = Very Soft 6 = Very Hard '0 0' = Soft '1 0' = Normal '2 0' = Hard
> 0x0022 | WorldTimeLocation | int16u | 0 = Hometown 1 = Destination
> 0x0023 | HometownCity | int16u | --> Pentax City Values
> 0x0024 | DestinationCity | int16u | --> Pentax City Values
> 0x0025 | HometownDST | int16u | 0 = No 1 = Yes
> 0x0026 | DestinationDST | int16u | 0 = No 1 = Yes
> 0x0029 | FrameNumber | int32u |
> 0x0032 | ImageProcessing | undef[4] | '0 0' = Unprocessed '0 0 0 0' = Unprocessed '0 0 0 4' = Digital Filter '2 0 0 0' = Cropped '4 0 0 0' = Color Filter '16 0 0 0' = Frame Synthesis?

> 0x0033

> PictureMode

> int8u[3]

> '0 0 0' = Program
> '0 0 1' = Program
> '0 4 0' = Standard
> '0 5 0' = Portrait
> '0 6 0' = Landscape
> '0 7 0' = Macro
> '0 8 0' = Sport
> '0 9 0' = Night Scene Portrait
> '0 10 0' = No Flash
> '0 11 0' = Night Scene
> '0 12 0' = Surf & Snow
> '0 13 0' = Text
> '0 14 0' = Sunset
> '0 15 0' = Kids
> '0 16 0' = Pet
> '0 17 0' = Candlelight
> '0 18 0' = Museum
> '1 4 0' = Auto PICT (Standard)
> '1 5 0' = Auto PICT (Portrait)
> '1 6 0' = Auto PICT (Landscape)
> '1 7 0' = Auto PICT (Macro)
> '1 8 0' = Auto PICT (Sport)
> '2 0 0' = Program AE
> '2 0 1' = Program AE
> '2 1 1' = Hi-speed Program
> '2 2 1' = DOF Program
> '2 3 1' = MTF Program
> '3 0 0' = Green Mode
> '3 0 1' = Green Mode
> '4 0 0' = Shutter Speed Priority
> '4 0 1' = Shutter Speed Priority
> '5 0 0' = Aperture Priority
> '5 0 1' = Aperture Priority
> '6 0 1' = Program Tv Shift
> '7 0 1' = Program Av Shift
> '8 0 0' = Manual
> '8 0 1' = Manual
> '9 0 0' = Bulb
> '9 0 1' = Bulb
> '10 0 1' = Aperture Priority (Off-Auto-Aperture)
> '11 0 1' = Manual (Off-Auto-Aperture)
> '12 0 1' = Bulb (Off-Auto-Aperture)
> '13 0 0' = Shutter & Aperture Priority AE
> '13 0 1' = Shutter & Aperture Priority AE (1)
> '15 0 0' = Sensitivity Priority AE
> '15 0 1' = Sensitivity Priority AE (1)
> '16 0 0' = Flash X-Sync Speed AE
> '16 0 1' = Flash X-Sync Speed AE (1)

> 0x0034 | DriveMode | int8u[4] | '0 0 0 0' = Single-frame '0 0 0 1' = Multiple Exposure '0 0 1 0' = Remote Control? '0 1 0 0' = Self-timer (12 sec) '0 2 0 0' = Self-timer (2 sec) '1 0 0 0' = Continuous
> 0x0037 | ColorSpace | int16u | 0 = sRGB 1 = Adobe RGB
> 0x0038 | ImageAreaOffset | int16u[2] |
> 0x0039 | RawImageSize | int16u[2]~ |
> 0x003c | AFPointsInFocus | N | (*istD only) Bit 0 = Upper-left Bit 1 = Top Bit 2 = Upper-right Bit 3 = Left Bit 4 = Mid-left Bit 5 = Center Bit 6 = Mid-right Bit 7 = Right Bit 8 = Lower-left Bit 9 = Bottom Bit 10 = Lower-right
> 0x003f | LensType | int8u[2] | --> Pentax LensType Values
> 0x0047 | CameraTemperature | int8s |
> 0x0049 | NoiseReduction | int16u | 0 = Off 1 = On
> 0x004d | FlashExposureComp | int32s |
> 0x004f | ImageTone | int16u | 0 = Natural 1 = Bright
> 0x005c | ShakeReductionInfo | - | --> Pentax SRInfo Tags
> 0x005d | ShutterCount | undef[4] | (raw value is a big-endian 4-byte integer, encrypted using Date and Time)
> 0x0200 | BlackPoint | int16u[4] |
> 0x0201 | WhitePoint | int16u[4] |
> 0x0206 | AEInfo | - | --> Pentax AEInfo Tags
> 0x0207 | LensInfo | - | --> Pentax LensInfo Tags
> 0x0208 | FlashInfo | - | --> Pentax FlashInfo Tags
> 0x0209 | AEMeteringSegments | int8u[16] | (measurements from each of the 16 AE metering segments, converted to LV)
> 0x020a | FlashADump? | Y |
> 0x020b | FlashBDump? | Y |
> 0x020d | WB_RGGBLevelsDaylight | int16u[4] |
> 0x020e | WB_RGGBLevelsShade | int16u[4] |
> 0x020f | WB_RGGBLevelsCloudy | int16u[4] |
> 0x0210 | WB_RGGBLevelsTungsten | int16u[4] |
> 0x0211 | WB_RGGBLevelsFluorescentD | int16u[4] |
> 0x0212 | WB_RGGBLevelsFluorescentN | int16u[4] |
> 0x0213 | WB_RGGBLevelsFluorescentW | int16u[4] |
> 0x0214 | WB_RGGBLevelsFlash | int16u[4] |
> 0x0215 | CameraInfo | - | --> Pentax CameraInfo Tags
> 0x0216 | BatteryInfo | - | --> Pentax BatteryInfo Tags
> 0x021f | AFInfo | - | --> Pentax AFInfo Tags
> 0x03fe | DataDump | N |
> 0x0402 | ToneCurve | Y~ |
> 0x0403 | ToneCurves | Y~ |
> 0x0e00 | PrintIM | - | --> PrintIM Tags

## Pentax PentaxModelID Values

> Value | PentaxModelID | Value | PentaxModelID
> --- | --- | --- | ---
> 0xd | = Optio 330/430 | 0x12b4c | = Optio WPi
> 0x12926 | = Optio 230 | 0x12b56 | = BenQ DC X600
> 0x12958 | = Optio 330GS | 0x12b60 | = *ist DS2
> 0x12962 | = Optio 450/550 | 0x12b62 | = Samsung GX-1S
> 0x1296c | = Optio S | 0x12b6a | = Optio A10
> 0x12994 | = *ist D | 0x12b7e | = *ist DL2
> 0x129b2 | = Optio 33L | 0x12b80 | = Samsung GX-1L
> 0x129bc | = Optio 33LF | 0x12b9c | = K100D
> 0x129c6 | = Optio 33WR/43WR/555 | 0x12b9d | = K110D
> 0x129d5 | = Optio S4 | 0x12ba2 | = K100D Super
> 0x12a02 | = Optio MX | 0x12bb0 | = Optio T10/T20
> 0x12a0c | = Optio S40 | 0x12be2 | = Optio W10
> 0x12a16 | = Optio S4i | 0x12bf6 | = Optio M10
> 0x12a34 | = Optio 30 | 0x12c1e | = K10D
> 0x12a52 | = Optio S30 | 0x12c20 | = Samsung GX10
> 0x12a66 | = Optio 750Z | 0x12c28 | = Optio S7
> 0x12a70 | = Optio SV | 0x12c2d | = Optio L20
> 0x12a75 | = Optio SVi | 0x12c32 | = Optio M20
> 0x12a7a | = Optio X | 0x12c3c | = Optio W20
> 0x12a8e | = Optio S5i | 0x12c46 | = Optio A20
> 0x12a98 | = Optio S50 | 0x12c78 | = Optio E30
> 0x12aa2 | = *ist DS | 0x12c82 | = Optio T30
> 0x12ab6 | = Optio MX4 | 0x12c8c | = Optio M30
> 0x12ac0 | = Optio S5n | 0x12c96 | = Optio W30
> 0x12aca | = Optio WP | 0x12ca0 | = Optio A30
> 0x12afc | = Optio S55 | 0x12cb4 | = Optio E40
> 0x12b10 | = Optio S5z | 0x12cbe | = Optio M40
> 0x12b1a | = *ist DL | 0x12cc8 | = Optio Z10
> 0x12b24 | = Optio S60 | 0x12cdc | = Optio S10
> 0x12b2e | = Optio S45 | 0x12ce6 | = Optio A40
> 0x12b38 | = Optio S6 | 0x12cf0 | = Optio V10

## Pentax City Values

> Value | City | Value | City | Value | City
> --- | --- | --- | --- | --- | ---
> 0 | = Pago Pago | 24 | = Berlin | 48 | = Hong Kong
> 1 | = Honolulu | 25 | = Johannesburg | 49 | = Perth
> 2 | = Anchorage | 26 | = Istanbul | 50 | = Beijing
> 3 | = Vancouver | 27 | = Cairo | 51 | = Shanghai
> 4 | = San Fransisco | 28 | = Jerusalem | 52 | = Manila
> 5 | = Los Angeles | 29 | = Moscow | 53 | = Taipei
> 6 | = Calgary | 30 | = Jeddah | 54 | = Seoul
> 7 | = Denver | 31 | = Tehran | 55 | = Adelaide
> 8 | = Mexico City | 32 | = Dubai | 56 | = Tokyo
> 9 | = Chicago | 33 | = Karachi | 57 | = Guam
> 10 | = Miami | 34 | = Kabul | 58 | = Sydney
> 11 | = Toronto | 35 | = Male | 59 | = Noumea
> 12 | = New York | 36 | = Delhi | 60 | = Wellington
> 13 | = Santiago | 37 | = Colombo | 61 | = Auckland
> 14 | = Caracus | 38 | = Kathmandu | 62 | = Lima
> 15 | = Halifax | 39 | = Dacca | 63 | = Dakar
> 16 | = Buenos Aires | 40 | = Yangon | 64 | = Algiers
> 17 | = Sao Paulo | 41 | = Bangkok | 65 | = Helsinki
> 18 | = Rio de Janeiro | 42 | = Kuala Lumpur | 66 | = Athens
> 19 | = Madrid | 43 | = Vientiane | 67 | = Nairobi
> 20 | = London | 44 | = Singapore | 68 | = Amsterdam
> 21 | = Paris | 45 | = Phnom Penh | 69 | = Stockholm
> 22 | = Milan | 46 | = Ho Chi Minh | 70 | = Lisbon
> 23 | = Rome | 47 | = Jakarta |  |

## Pentax LensType Values

> Value | LensType
> --- | ---
> '0 0' | = M-42 or No Lens
> '1 0' | = K,M Lens
> '2 0' | = A Series Lens
> '3 0' | = SIGMA
> '3 17' | = smc PENTAX-FA SOFT 85mm F2.8
> '3 18' | = smc PENTAX-F 1.7X AF ADAPTER
> '3 19' | = smc PENTAX-F 24-50mm F4
> '3 20' | = smc PENTAX-F 35-80mm F4-5.6
> '3 21' | = smc PENTAX-F 80-200mm F4.7-5.6
> '3 22' | = smc PENTAX-F FISH-EYE 17-28mm F3.5-4.5
> '3 23' | = smc PENTAX-F 100-300mm F4.5-5.6
> '3 24' | = smc PENTAX-F 35-135mm F3.5-4.5
> '3 25' | = smc PENTAX-F 35-105mm F4-5.6 or SIGMA or Tokina
> '3 26' | = smc PENTAX-F* 250-600mm F5.6 ED[IF]
> '3 27' | = smc PENTAX-F 28-80mm F3.5-4.5
> '3 28' | = smc PENTAX-F 35-70mm F3.5-4.5
> '3 29' | = PENTAX-F 28-80mm F3.5-4.5 or SIGMA AF 18-125mm F3.5-5.6 DC
> '3 30' | = PENTAX-F 70-200mm F4-5.6
> '3 31' | = smc PENTAX-F 70-210mm F4-5.6
> '3 32' | = smc PENTAX-F 50mm F1.4
> '3 33' | = smc PENTAX-F 50mm F1.7
> '3 34' | = smc PENTAX-F 135mm F2.8 [IF]
> '3 35' | = smc PENTAX-F 28mm F2.8
> '3 36' | = SIGMA 20mm F1.8 EX DG ASPHERICAL RF
> '3 38' | = smc PENTAX-F* 300mm F4.5 ED[IF]
> '3 39' | = smc PENTAX-F* 600mm F4 ED[IF]
> '3 40' | = smc PENTAX-F MACRO 100mm F2.8
> '3 41' | = smc PENTAX-F MACRO 50mm F2.8 or Sigma 50mm F2,8 MACRO
> '3 44' | = Tamron 35-90mm F4 AF or various SIGMA models
> '3 46' | = SIGMA APO 70-200mm F2.8 EX
> '3 50' | = smc PENTAX-FA 28-70mm F4 AL
> '3 51' | = SIGMA 28mm F1.8 EX DG ASPHERICAL MACRO
> '3 52' | = smc PENTAX-FA 28-200mm F3.8-5.6 AL[IF]
> '3 53' | = smc PENTAX-FA 28-80mm F3.5-5.6 AL
> '3 247' | = smc PENTAX-DA FISH-EYE 10-17mm F3.5-4.5 ED[IF]
> '3 248' | = smc PENTAX-DA 12-24mm F4 ED AL[IF]
> '3 250' | = smc PENTAX-DA 50-200mm F4-5.6 ED
> '3 251' | = smc PENTAX-DA 40mm F2.8 Limited
> '3 252' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL
> '3 253' | = smc PENTAX-DA 14mm F2.8 ED[IF]
> '3 254' | = smc PENTAX-DA 16-45mm F4 ED AL
> '3 255' | = SIGMA
> '4 1' | = smc PENTAX-FA SOFT 28mm F2.8
> '4 2' | = smc PENTAX-FA 80-320mm F4.5-5.6
> '4 3' | = smc PENTAX-FA 43mm F1.9 Limited
> '4 6' | = smc PENTAX-FA 35-80mm F4-5.6
> '4 12' | = smc PENTAX-FA 50mm F1.4
> '4 15' | = smc PENTAX-FA 28-105mm F4-5.6 [IF]
> '4 16' | = TAMRON AF 80-210mm F4-5.6 (178D)
> '4 19' | = TAMRON SP AF 90mm F2.8 (172E)
> '4 20' | = smc PENTAX-FA 28-80mm F3.5-5.6
> '4 22' | = TOKINA 28-80mm F3.5-5.6
> '4 23' | = smc PENTAX-FA 20-35mm F4 AL
> '4 24' | = smc PENTAX-FA 77mm F1.8 Limited
> '4 25' | = TAMRON SP AF 14mm F2.8
> '4 26' | = smc PENTAX-FA MACRO 100mm F3.5
> '4 27' | = TAMRON AF28-300mm F/3.5-6.3 LD Aspherical[IF] MACRO (285D)
> '4 28' | = smc PENTAX-FA 35mm F2 AL
> '4 29' | = TAMRON AF 28-200mm F/3.8-5.6 LD Super II MACRO (371D)
> '4 34' | = smc PENTAX-FA 24-90mm F3.5-4.5 AL[IF]
> '4 35' | = smc PENTAX-FA 100-300mm F4.7-5.8
> '4 36' | = TAMRON AF70-300mm F/4-5.6 LD MACRO
> '4 37' | = TAMRON SP AF 24-135mm F3.5-5.6 AD AL (190D)
> '4 38' | = smc PENTAX-FA 28-105mm F3.2-4.5 AL[IF]
> '4 39' | = smc PENTAX-FA 31mm F1.8AL Limited
> '4 41' | = TAMRON AF 28-200mm Super Zoom F3.8-5.6 Aspherical XR [IF] MACRO (A03)
> '4 43' | = smc PENTAX-FA 28-90mm F3.5-5.6
> '4 44' | = smc PENTAX-FA J 75-300mm F4.5-5.8 AL
> '4 45' | = TAMRON 28-300mm F3.5-6.3 Ultra zoom XR
> '4 46' | = smc PENTAX-FA J 28-80mm F3.5-5.6 AL
> '4 47' | = smc PENTAX-FA J 18-35mm F4-5.6 AL
> '4 49' | = TAMRON SP AF 28-75mm F2.8 XR Di (A09)
> '4 51' | = smc PENTAX-D FA 50mm F2.8 MACRO
> '4 52' | = smc PENTAX-D FA 100mm F2.8 MACRO
> '4 244' | = smc PENTAX-DA 21mm F3.2 AL Limited
> '4 245' | = Schneider D-XENON 50-200mm
> '4 246' | = Schneider D-XENON 18-55mm
> '4 247' | = smc PENTAX-DA 10-17mm F3.5-4.5 ED [IF] Fisheye zoom
> '4 248' | = smc PENTAX-DA 12-24mm F4 ED AL [IF]
> '4 249' | = TAMRON XR DiII 18-200mm F3.5-6.3 (A14)
> '4 250' | = smc PENTAX-DA 50-200mm F4-5.6 ED
> '4 251' | = smc PENTAX-DA 40mm F2.8 Limited
> '4 252' | = smc PENTAX-DA 18-55mm F3.5-5.6 AL
> '4 253' | = smc PENTAX-DA 14mm F2.8 ED[IF]
> '4 254' | = smc PENTAX-DA 16-45mm F4 ED AL
> '5 1' | = smc PENTAX-FA* 24mm F2 AL[IF]
> '5 2' | = smc PENTAX-FA 28mm F2.8 AL
> '5 3' | = smc PENTAX-FA 50mm F1.7
> '5 4' | = smc PENTAX-FA 50mm F1.4
> '5 5' | = smc PENTAX-FA* 600mm F4 ED[IF]
> '5 6' | = smc PENTAX-FA* 300mm F4.5 ED[IF]
> '5 7' | = smc PENTAX-FA 135mm F2.8 [IF]
> '5 8' | = smc PENTAX-FA MACRO 50mm F2.8
> '5 9' | = smc PENTAX-FA MACRO 100mm F2.8
> '5 10' | = smc PENTAX-FA* 85mm F1.4 [IF]
> '5 11' | = smc PENTAX-FA* 200mm F2.8 ED[IF]
> '5 12' | = smc PENTAX-FA 28-80mm F3.5-4.7
> '5 13' | = smc PENTAX-FA 70-200mm F4-5.6
> '5 14' | = smc PENTAX-FA* 250-600mm F5.6 ED[IF]
> '5 15' | = smc PENTAX-FA 28-105mm F4-5.6
> '5 16' | = smc PENTAX-FA 100-300mm F4.5-5.6
> '6 1' | = smc PENTAX-FA* 85mm F1.4[IF]
> '6 2' | = smc PENTAX-FA* 200mm F2.8 ED[IF]
> '6 3' | = smc PENTAX-FA* 300mm F2.8 ED[IF]
> '6 4' | = smc PENTAX-FA* 28-70mm F2.8 AL
> '6 5' | = smc PENTAX-FA* 80-200mm F2.8 ED[IF]
> '6 6' | = smc PENTAX-FA* 28-70mm F2.8 AL
> '6 7' | = smc PENTAX-FA* 80-200mm F2.8 ED[IF]
> '6 8' | = smc PENTAX-FA 28-70mm F4AL
> '6 9' | = smc PENTAX-FA 20mm F2.8
> '6 10' | = smc PENTAX-FA* 400mm F5.6 ED[IF]
> '6 13' | = smc PENTAX-FA* 400mm F5.6 ED[IF]
> '6 14' | = smc PENTAX-FA* MACRO 200mm F4 ED[IF]
> '7 0' | = smc PENTAX-DA 21mm F3.2 AL Limited
> '7 238' | = TAMRON AF 18-250mm F3.5-6.3 Di II LD Aspherical [IF] MACRO
> '7 243' | = smc PENTAX-DA 70mm F2.4 Limited
> '7 244' | = smc PENTAX-DA 21mm F3.2 AL Limited
> '8 241' | = smc PENTAX-DA* 50-135mm F2.8 ED [IF] SDM
> '8 242' | = smc PENTAX-DA* 16-50mm F2.8 ED AL [IF] SDM

## Pentax SRInfo Tags

Shake reduction information.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SRResult | int8u | 0 = Not stabilized Bit 0 = Stabilized Bit 6 = Not ready
> 1 | ShakeReduction | int8u | 0 = Off 1 = On
> 2 | SR_SWSToSWRTime | int8u | (time from when the shutter button was half pressed to when the shutter was released)

## Pentax AEInfo Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AEExposureTime | int8u | (val = 24 * 2**((32-raw)/8))
> 1 | AEAperture | int8u | (val = (2**((raw-4)/16)) / 16)
> 2 | AE_ISO | int8u | (val = 100 * 2**((raw-32)/8))
> 3 | AEXv | int8u | (val = (raw-64)/8)
> 4 | AEBXv | int8s | (val = raw / 8)
> 5 | AEFlashTv | int8u | (val = 24 * 2**((32-raw)/8))
> 6 | AEProgramMode | int8u | 0 = Manual/Program AE 1 = Aperture Priority/Bulb 2 = Shutter Speed Priority 3 = Program 35 = Standard 43 = Portrait 51 = Landscape 59 = Macro 67 = Sport 75 = Night Scene Portrait 83 = No Flash 91 = Night Scene 99 = Surf & Snow 107 = Text 115 = Sunset 123 = Kids 131 = Pet 139 = Candlelight 147 = Museum
> 7 | AEExtra? | int8u |

## Pentax LensInfo Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensType | N | --> Pentax LensType Values (for most models the first 2 bytes are LensType, but for the K10D the decoding is a bit different)
> 4 | LensCodes | int8u[16] | (all models but the K10D)
> 5 | LensCodes | int8u[16] | (K10D only)

## Pentax FlashInfo Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FlashStatus | int8u |
> 1 | FlashModeCode | int8u | 149 = On, Wireless 192 = On 193 = On, Red-eye reduction 194 = Auto, Fired 200 = On, Slow-sync 201 = On, Slow-sync, Red-eye reduction 202 = On, Trailing-curtain Sync 240 = Off (240) 241 = Off (241) 242 = Off (242) 244 = Off (244)
> 2 | ExternalFlashMode | int8u |
> 3 | InternalFlashMagni | int8u |
> 4 | TTL_DA_AUp | int8u |
> 5 | TTL_DA_ADown | int8u |
> 6 | TTL_DA_BUp | int8u |
> 7 | TTL_DA_BDown | int8u |

## Pentax CameraInfo Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PentaxModelID | int32u | --> Pentax PentaxModelID Values
> 1 | ManufactureDate | int32u |
> 2 | ModelRevision | int32u[2] |
> 4 | InternalSerialNumber | int32u |

## Pentax BatteryInfo Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | BatteryType | int8u |
> 1 | BatteryBodyGripStates | int8u | (body and grip battery state)
> 2 | BatteryADBodyNoLoad | int8u |
> 3 | BatteryADBodyLoad | int8u |
> 4 | BatteryADGripNoLoad | int8u |
> 5 | BatteryADGripLoad | int8u |

## Pentax AFInfo Tags

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---

> 11

> AFPointsInFocus

> int8u

> (may report two points in focus even though a single AFPoint has been selected, in which case the selected AFPoint is the first reported)
> 0 = None
> 1 = Lower-left, Bottom
> 2 = Bottom
> 3 = Lower-right, Bottom
> 4 = Mid-left, Center
> 5 = Center (horizontal)
> 6 = Mid-right, Center
> 7 = Upper-left, Top
> 8 = Top
> 9 = Upper-right, Top
> 10 = Right
> 11 = Lower-left, Mid-left
> 12 = Upper-left, Mid-left
> 13 = Bottom, Center
> 14 = Top, Center
> 15 = Lower-right, Mid-right
> 16 = Upper-right, Mid-right
> 17 = Left
> 18 = Mid-left
> 19 = Center (vertical)
> 20 = Mid-right

## Pentax Type2 Tags

These tags are used by the Pentax Optio 330 and 430, and are similar to the tags used by Casio.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | RecordingMode | int16u | 0 = Auto 1 = Night Scene 2 = Manual
> 0x0002 | Quality | int16u | 0 = Good 1 = Better 2 = Best
> 0x0003 | FocusMode | int16u | 2 = Custom 3 = Auto
> 0x0004 | FlashMode | int16u | 1 = Auto 2 = On 4 = Off 6 = Red-eye reduction
> 0x0007 | WhiteBalance | int16u | 0 = Auto 1 = Daylight 2 = Shade 3 = Tungsten 4 = Fluorescent 5 = Manual
> 0x000a | DigitalZoom | int32u |
> 0x000b | Sharpness | int16u | 0 = Normal 1 = Soft 2 = Hard
> 0x000c | Contrast | int16u | 0 = Normal 1 = Low 2 = High
> 0x000d | Saturation | int16u | 0 = Normal 1 = Low 2 = High
> 0x0014 | ISO | int16u | 10 = 100 16 = 200 50 = 50 100 = 100 200 = 200 400 = 400 800 = 800 1600 = 1600 3200 = 3200
> 0x0017 | ColorFilter | int16u | 1 = Full 2 = Black & White 3 = Sepia
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x1000 | HometownCityCode | undef[4] |
> 0x1001 | DestinationCityCode | undef[4] |

## Pentax Type4 Tags

The following few tags are extracted from the wealth of information available in maker notes of the Optio E20. These maker notes are stored as ASCII text in a format very similar to some HP models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'F/W Version' | FirmwareVersion | N |

## Pentax MOV Tags

This information is found in Pentax MOV video images.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | N |
> 38 | ExposureTime | N |
> 42 | FNumber | N |
> 50 | ExposureCompensation | N |
> 68 | WhiteBalance | N | 0 = Auto 1 = Daylight 2 = Shade 3 = Fluorescent 4 = Tungsten 5 = Manual
> 72 | FocalLength | N |
> 175 | ISO | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Oct 23, 2007

<-- ExifTool Tag Names