## Panasonic Tags

Panasonic tags are also used for Leica cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | ImageQuality | int16u | 2 = High 3 = Normal 6 = Very High 7 = Raw 9 = Motion Picture
> 0x0002 | FirmwareVersion | undef | (for some camera models such as the FZ30 this may be an internal production reference number and not the actual firmware version)
> 0x0003 | WhiteBalance | int16u | 1 = Auto 2 = Daylight 3 = Cloudy 4 = Halogen 5 = Manual 8 = Flash 10 = Black & White 11 = Manual
> 0x0007 | FocusMode | int16u | 1 = Auto 2 = Manual 4 = Auto, Focus button 5 = Auto, Continuous
> 0x000f | AFMode | int8u[2] | 16 = Normal? '0 1' = Spot Mode On '0 16' = Spot Mode Off or 3-area (high speed) '1 0' = Spot Focusing '1 1' = 5-area '16 0' = 1-area '16 16' = 1-area (high speed) '32 0' = 3-area (auto)? '32 1' = 3-area (left)? '32 2' = 3-area (center)? '32 3' = 3-area (right)?
> 0x001a | ImageStabilization | int16u | 2 = On, Mode 1 3 = Off 4 = On, Mode 2
> 0x001c | MacroMode | int16u | 1 = On 2 = Off 257 = Tele-Macro

> 0x001f

> ShootingMode

> int16u

> 1 = Normal
> 2 = Portrait
> 3 = Scenery
> 4 = Sports
> 5 = Night Portrait
> 6 = Program
> 7 = Aperture Priority
> 8 = Shutter Priority
> 9 = Macro
> 11 = Manual
> 12 = Movie Preview
> 13 = Panning
> 14 = Simple
> 18 = Fireworks
> 19 = Party
> 20 = Snow
> 21 = Night Scenery
> 22 = Food
> 23 = Baby
> 24 = Soft Skin
> 25 = Candlelight
> 26 = Starry Night
> 27 = High Sensitivity
> 29 = Underwater
> 30 = Beach
> 31 = Aerial Photo
> 32 = Sunset
> 33 = Pet
> 34 = Intelligent ISO

> 0x0020 | Audio | int16u | 1 = Yes 2 = No
> 0x0021 | DataDump | N |
> 0x0023 | WhiteBalanceBias | int16s |
> 0x0024 | FlashBias | int16s |
> 0x0025 | InternalSerialNumber | undef[16] | (this number is unique, and contains the date of manufacture, but is not the same as the number printed on the camera body)
> 0x0026 | PanasonicExifVersion | undef |
> 0x0028 | ColorEffect | int16u | 1 = Off 2 = Warm 3 = Cool 4 = Black & White 5 = Sepia
> 0x0029 | TimeSincePowerOn | int32u | (time in 1/100 sec from when the camera was powered on to when the image is written to memory card)
> 0x002a | BurstMode | int16u | 0 = Off 1 = Low/High Quality 2 = Infinite
> 0x002b | SequenceNumber | int32u |
> 0x002c | Contrast | int16u | 0x0 = Normal 0x1 = Low 0x2 = High 0x100 = Low 0x110 = Normal 0x120 = High
> 0x002d | NoiseReduction | int16u | 0 = Standard 1 = Low 2 = High
> 0x002e | SelfTimer | int16u | 1 = Off 2 = 10s 3 = 2s
> 0x0030 | Rotation | int16u | 1 = Horizontal (normal) 6 = Rotate 90 CW 8 = Rotate 270 CW
> 0x0032 | ColorMode | int16u | 0 = Normal 1 = Natural
> 0x0033 | BabyAge | string | (or pet age)
> 0x0034 | OpticalZoomMode | int16u | 1 = Standard 2 = EX Optics
> 0x0035 | ConversionLens | int16u | 1 = Off 2 = Wide 3 = Telephoto 4 = Macro
> 0x0036 | TravelDay | int16u |
> 0x003a | WorldTimeLocation | int16u | 1 = Home 2 = Destination
> 0x003c | ProgramISO | int16u |
> 0x0042 | FilmMode | int16u | 1 = Standard (color) 2 = Dynamic (color) 3 = Nature (color) 4 = Smooth (color) 5 = Standard (B&W) 6 = Dynamic (B&W) 7 = Smooth (B&W)
> 0x0046 | WBAdjustAB | int16u | (positive is a shift toward blue)
> 0x0047 | WBAdjustGM | int16u | (positive is a shift toward green)
> 0x0051 | LensType | string |
> 0x0052 | LensSerialNumber | string |
> 0x0053 | AccessoryType | string |
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x8000 | MakerNoteVersion | undef |

> 0x8001

> SceneMode

> int16u

> 0 = Off
> 1 = Normal
> 2 = Portrait
> 3 = Scenery
> 4 = Sports
> 5 = Night Portrait
> 6 = Program
> 7 = Aperture Priority
> 8 = Shutter Priority
> 9 = Macro
> 11 = Manual
> 12 = Movie Preview
> 13 = Panning
> 14 = Simple
> 18 = Fireworks
> 19 = Party
> 20 = Snow
> 21 = Night Scenery
> 22 = Food
> 23 = Baby
> 24 = Soft Skin
> 25 = Candlelight
> 26 = Starry Night
> 27 = High Sensitivity
> 29 = Underwater
> 30 = Beach
> 31 = Aerial Photo
> 32 = Sunset
> 33 = Pet
> 34 = Intelligent ISO

> 0x8004 | WBRedLevel | int16u |
> 0x8005 | WBGreenLevel | int16u |
> 0x8006 | WBBlueLevel | int16u |
> 0x8010 | BabyAge | string | (or pet age)

## Panasonic Type2 Tags

This type of maker notes is used by models such as the NV-DS65, PV-D2002, PV-DC3000, PV-DV203, PV-DV401, PV-DV702, PV-L2001, PV-SD4090, PV-SD5000 and iPalm.

> Index | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MakerNoteType | N |
> 3 | Gain | N |

## Panasonic Raw Tags

These tags are found in IFD0 of Panasonic RAW images.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | PanasonicRawVersion | undef |
> 0x0002 | SensorWidth | N |
> 0x0003 | SensorHeight | N |
> 0x0004 | SensorTopBorder | N |
> 0x0005 | SensorLeftBorder | N |
> 0x0006 | ImageHeight | N |
> 0x0007 | ImageWidth | N |
> 0x0011 | RedBalance | int16u | (found in Digilux 2 RAW images)
> 0x0012 | BlueBalance | int16u |
> 0x0017 | ISO | int16u |
> 0x0024 | WBRedLevel | int16u |
> 0x0025 | WBGreenLevel | int16u |
> 0x0026 | WBBlueLevel | int16u |
> 0x010f | Make | string |
> 0x0110 | Model | string |
> 0x0111 | StripOffsets | N |
> 0x0112 | Orientation | int16u | 1 = Horizontal (normal) 2 = Mirror horizontal 3 = Rotate 180 4 = Mirror vertical 5 = Mirror horizontal and rotate 270 CW 6 = Rotate 90 CW 7 = Mirror horizontal and rotate 90 CW 8 = Rotate 270 CW
> 0x0116 | RowsPerStrip | N |
> 0x0117 | StripByteCounts | N |
> 0x8769 | ExifOffset | - | --> EXIF Tags
> 0x8825 | GPSInfo | - | --> GPS Tags

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Aug 30, 2007

<-- ExifTool Tag Names