/////////////////////////////////////////////////////////////////////////////////////////////////////////////////
//// This example is from the ACE Programmers Guide.
//// Chapter: "IPC SAP" (Interprocess Communication Mechanisms in ACE).
//// For details please see the guide at
//// http://www.cs.wustl.edu/~schmidt/ACE.html
//// AUTHOR: Umar Syyid (usyyid@hns.com)
//// and Ambreen Ilyas (ambreen@bitsmart.com)
/////////////////////////////////////////////////////////////////////////////////////////////////////////////

//Example 4
//Client
#include "ace/OS.h"
#include "ace/SOCK_Dgram.h"
#include "ace/INET_Addr.h"

#define DATA_BUFFER_SIZE 1024
#define SIZE_DATA 28
class Client{
public:
Client(char * remote_addr,int port)
:remote_addr_(remote_addr),
local_addr_((u_short)0),local_(local_addr_){
data_buf = new char[DATA_BUFFER_SIZE];
remote_addr_.set_port_number(port);
}
//Accept data from the remote host using the datgram component local_
int accept_data(){
if(local_.recv(data_buf,DATA_BUFFER_SIZE,remote_addr_)!=-1){
ACE_DEBUG((LM_DEBUG, "Data received from remote server %s
was: %s \n" ,remote_addr_.get_host_name(), data_buf));
return 0;
}
else
return -1;
}

//Send data to the remote. Once data has been sent wait for a reply from
//the server.
int send_data(){
ACE_DEBUG((LM_DEBUG,"Preparing to send data to server %s:%d\n",
remote_addr_.get_host_name(),remote_addr_.get_port_number()));
ACE_OS::strcpy(data_buf,"Client says hello");
while(local_.send
(data_buf,ACE_OS::strlen(data_buf)+1,remote_addr_)!=-1){
ACE_OS::sleep(1);
if(accept_data()==-1)
break;
}
return -1;
}

private:
char *data_buf;
ACE_INET_Addr remote_addr_;
ACE_INET_Addr local_addr_;
ACE_SOCK_Dgram local_;
};

int main(int argc, char *argv[]){
if(argc<3){
ACE_OS::printf("Usage: Client hostname port_number \n");
ACE_OS::exit(1);
}
Client client(argv[1],ACE_OS::atoi(argv[2]));
client.send_data();
return 0;
}
Next Example