NTPDSIM(1)

NAME
ntpdsim - NTP daemon simulation program

SYNOPSIS
ntpdsim [-flag [value]]... [--opt-name [[=| ]value]]...

All arguments must be options.

DESCRIPTION
This manual page documents, briefly, the ntpdsim command.

OPTIONS

-4, --ipv4
    Force IPv4 DNS name resolution. This option is a member of the ipv4 class of options.

    Force DNS resolution of following host names on the command line to the IPv4 namespace.

-6, --ipv6
    Force IPv6 DNS name resolution. This option is a member of the ipv4 class of options.

    Force DNS resolution of following host names on the command line to the IPv6 namespace.

-a, --authreq
    Require crypto authentication. This option must not appear in combination with any of the following options: authnoreq.

    Require cryptographic authentication for broadcast client, multicast client and symmetric passive associations. This is the default.

-A, --authnoreq
    Do not require crypto authentication. This option must not appear in combination with any of the following options: authreq.

    Do not require cryptographic authentication for broadcast client, multicast client and symmetric passive associations. This is almost never a good idea.

-b, --bcastsync
    Allow us to sync to broadcast servers.

-B string, --simbroadcastdelay=string
    Simulator broadcast delay.

-c string, --configfile=string
    configuration file name.

    The name and path of the configuration file, /etc/ntp.conf by default.

-C string, --phasenoise=string
    Phase noise level.

-d, --debug-level
    Increase output debug message level. This option may appear an unlimited number of times.

    Increase the debugging message output level.

-D string, --set-debug-level=string
    Set the output debug message level. This option may appear an unlimited number of times.

    Set the output debugging level. Can be supplied multiple times, but each overrides the previous value(s).

-f string, --driftfile=string
    frequency drift file name.

    The name and path of the frequency file, /etc/ntp.drift by default. This is the same operation as the driftfile driftfile configuration specification in the /etc/ntp.conf file.

-g, --panicgate
    Allow the first adjustment to be Big.

    Normally, ntpd exits with a message to the system log if the offset exceeds the panic threshold, which is 1000 s by default. This option allows the time to be set to any value without restriction; however, this can happen only once. If the threshold is exceeded after that, ntpd will exit with a message to the system log. This option can be used with the -q and -x options. See the tinker configuration file directive for other options.

-H string, --simslew=string
    Simuator slew.

-i string, --jaildir=string
    Jail directory.

    Chroot the server to the directory jaildir This option also implies that the server attempts to drop root privileges at startup (otherwise, chroot gives very little additional security), and it is only available if the OS supports to run the server without full root privileges. You may need to also specify a -u option.

-I iface, --interface=iface
    Listen on interface. This option may appear an unlimited number of times.

-k string, --keyfile=string
    path to symmetric keys.

    Specify the name and path of the symmetric key file. /etc/ntp.keys is the default. This is the same operation as the keys keyfile configuration file directive.

-l string, --logfile=string
    path to the log file.

    Specify the name and path of the log file. The default is the system log file. This is the same operation as the logfile logfile configuration file directive.

-L, --novirtualips
    Do not listen to virtual IPs.

    Do not listen to virtual IPs. The default is to listen.

-M, --modifymmtimer
    Modify Multimedia Timer (Windows only).

    Set the Windows Multimedia Timer to highest resolution.

-n, --nofork
    Do not fork.

-N, --nice
    Run at high priority.

    To the extent permitted by the operating system, run ntpd at the highest priority.

-O string, --servertime=string
    Server time.

-p string, --pidfile=string
    path to the PID file.

    Specify the name and path of the file used to record ntpd's process ID. This is the same operation as the pidfile pidfile configuration file directive.

-P number, --priority=number
    Process priority. This option takes an integer number as its argument.

    To the extent permitted by the operating system, run ntpd at the specified sched_setscheduler(SCHED_FIFO) priority.

-q, --quit
    Set the time and quit.

    ntpd will exit just after the first time the clock is set. This behavior mimics that of the ntpdate program, which is to be retired. The -g and -x options can be used with this option. Note: The kernel time discipline is disabled with this option.

-r string, --propagationdelay=string
    Broadcast/propagation delay.

    Specify the default propagation delay from the broadcast/multicast server to this client. This is necessary only if the delay cannot be computed automatically by the protocol.

-U number, --updateinterval=number
    interval in seconds between scans for new or dropped interfaces. This option takes an integer number as its argument.

    Give the time in seconds between two scans for new or dropped interfaces. For systems with routing socket support the scans will be performed shortly after the interface change has been detected by the system. Use 0 to disable scanning.

-s string, --statsdir=string
    Statistics file location.

    Specify the directory path for files created by the statistics facility. This is the same operation as the statsdir statsdir configuration file directive.

-S string, --endsimtime=string
    Simulation end time.

-t tkey, --trustedkey=tkey
    Trusted key number. This option may appear an unlimited number of times.

    Add a key number to the trusted key list.

-T string, --freqerr=string
    Simulation frequency error.

-W string, --walknoise=string
    Simulation random walk noise.

-u string, --user=string
    Run as userid (or userid:groupid).

    Specify a user, and optionally a group, to switch to. This option is only available if the OS supports to run the server without full root privileges. Currently, this option is supported under NetBSD (configure with --enable-clockctl ) and Linux (configure with --enable-linuxcaps ).

-v nvar, --var=nvar
    make ARG an ntp variable (RW). This option may appear an unlimited number of times.

-V ndvar, --dvar=ndvar
    make ARG an ntp variable (RW|DEF). This option may appear an unlimited number of times.

-x, --slew
    Slew up to 600 seconds.

    Normally, the time is slewed if the offset is less than the step threshold, which is 128 ms by default, and stepped if above the threshold. This option sets the threshold to 600 s, which is well within the accuracy window to set the clock manually. Note: Since the slew rate of typical Unix kernels is limited to 0.5 ms/s, each second of adjustment requires an amortization interval of 2000 s. Thus, an adjustment as much as 600 s will take almost 14 days to complete. This option can be used with the -g and -q options. See the tinker configuration file directive for other options. Note: The kernel time discipline is disabled with this option.

-Y string, --ndelay=string
    Simulation network delay.

-Z string, --pdelay=string
    Simulation processing delay.

-?, --help
    Display usage information and exit.

-!, --more-help
    Extended usage information passed thru pager.

-> [rcfile], --save-opts[=rcfile]
    Save the option state to rcfile. The default is the last configuration file listed in the OPTION PRESETS section, below.

-< rcfile, --load-opts=rcfile, --no-load-opts
    Load options from rcfile. The no-load-opts form will disable the loading of earlier RC/INI files. --no-load-opts is handled early, out of order.

-v [{v|c|n}], --version[={v|c|n}]
    Output version of program and exit. The default mode is `v', a simple version. The `c' mode will print copyright information and `n' will print the full copyright notice.

OPTION PRESETS
Any option that is not marked as not presettable may be preset by loading values from configuration ("RC" or ".INI") file(s) and values from environment variables named:
  NTPDSIM_<option-name> or NTPDSIM
The environmental presets take precedence (are processed later than) the configuration files. The homerc files are "$HOME", and ".". If any of these are directories, then the file .ntprc is searched for within those directories.

AUTHOR
David L. Mills and/or others
Please send bug reports to: http://bugs.ntp.isc.org, bugs@ntp.org

see html/copyright.html

This manual page was AutoGen-erated from the ntpdsim option definitions.