SGE_PASSWD(1)              Grid Engine User Commands             SGE_PASSWD(1)



[1mNAME[0m
       sgepasswd - Modify the Grid Engine password file of Grid Engine

[1mSYNTAX[0m
       [1msgepasswd [22m[[ [1m-D domain [22m] [1m-d user [22m]

       [1msgepasswd [22m[ [1m-D domain [22m] [ [1muser [22m]

[1mDESCRIPTION[0m
       [4msgepasswd[24m modifies the Grid Engine password file [4msgepasswd[24m(5).

       This  file  contains  a  list  of usernames and their Microsoft Windows
       password in encrypted form.  [4mSee[24m(sge_execd)8 and [4msge_shepherd[24m(8) on how
       hosts  running Microsoft Windows as operating systems use this informa-
       tion to start jobs for a certain user.

       Each user can use the [4msgepasswd[24m application to  add  a  new  entry  for
       their  own user account. It is also possible to change the stored pass-
       word with [4msgepasswd[24m since the user knows the old one.

       The root user additionally has the permission to  change  the  password
       entries for other user accounts. Root can also delete existing entries.

       The [4msgepasswd[24m binary is only available on non-Windows hosts.


[1mOPTIONS[0m
       [1m-D domain[0m
              By default [4msgepasswd[24m will add/modify the current  Unix  username
              without  domain specification.  This switch can be used to add a
              domain specification in front of the current user name.  Consult
              your  Microsoft  Windows  documentation  to get more information
              about domain users.

       [1m-d user[0m
              Only root can use this parameter  to  delete  entries  from  the
              [4msgepasswd[24m(5) file.

       [1m-help  [22mPrints a listing of all options.

[1mENVIRONMENTAL VARIABLES[0m
       [1mSGE_CERTFILE   [22mSpecifies  the  location of public key file. Per default
                      [4msgepasswd[24m will  use  the  file  $SGE_ROOT/$SGE_CELL/com-
                      mon/sgeCA/certs/cert.pem

       [1mSGE_KEYFILE    [22mIf  set, specifies the location of the private key file.
                      Default     is     /var/sgeCA/port$SGE_QMASTER_PORT/pri-
                      vate/key.pem

[1mSEE ALSO[0m
       [4msge_intro[24m(1), [4msgepasswd[24m(5)

[1mCOPYRIGHT[0m
       See [4msge_intro[24m(1) for a full statement of rights and permissions.



GE 6.1                   $Date: 2007/07/19 08:17:16 $            SGE_PASSWD(1)
