#N canvas 10 49 705 610 12;
#X floatatom 262 549 0 0 0;
#N canvas 176 241 532 273 output 0;
#X obj 338 160 t b;
#X obj 338 110 f;
#X obj 338 60 inlet;
#X text 344 29 mute;
#X obj 338 185 f;
#X msg 425 178 0;
#X msg 338 85 bang;
#X obj 338 135 moses 1;
#X obj 398 111 moses 1;
#X obj 83 148 dbtorms;
#X obj 398 86 r master-lvl;
#X obj 83 42 r master-lvl;
#X obj 338 210 s master-lvl;
#X obj 17 148 inlet~;
#X obj 199 41 inlet;
#X text 199 18 level;
#X obj 199 100 s master-lvl;
#X msg 96 65 set \$1;
#X obj 96 89 outlet;
#X msg 214 64 \; pd dsp 1;
#X obj 83 194 line~;
#X obj 22 212 *~;
#X obj 22 241 dac~;
#X obj 83 171 pack 0 50;
#X text 15 125 audio;
#X text 93 110 show level;
#X obj 17 177 hip~ 1;
#X connect 0 0 4 0;
#X connect 1 0 7 0;
#X connect 2 0 6 0;
#X connect 4 0 12 0;
#X connect 5 0 12 0;
#X connect 6 0 1 0;
#X connect 7 0 0 0;
#X connect 7 1 5 0;
#X connect 8 1 4 1;
#X connect 9 0 23 0;
#X connect 10 0 1 1;
#X connect 10 0 8 0;
#X connect 11 0 9 0;
#X connect 11 0 17 0;
#X connect 13 0 26 0;
#X connect 14 0 16 0;
#X connect 14 0 19 0;
#X connect 17 0 18 0;
#X connect 20 0 21 1;
#X connect 21 0 22 0;
#X connect 21 0 22 1;
#X connect 23 0 20 0;
#X connect 26 0 21 0;
#X restore 226 576 pd output;
#X msg 302 549 MUTE;
#X msg 59 550 bang;
#X obj 185 427 cos~;
#X floatatom 232 217 4 0 0;
#X obj 232 241 / 10;
#X text 464 288 --- 0.02 seconds ---;
#X obj 185 397 *~;
#X text 236 133 center;
#X obj 232 313 line~;
#X obj 232 265 max 0;
#X graph graph3 0 -2 881 2 450 276 650 136;
#X array carrier 882 float 0;
#X pop;
#X floatatom 33 284 4 0 0;
#X text 29 240 fundamental;
#X text 31 2 ADDING TWO COSINES;
#X text 234 152 freq. (in;
#X text 233 171 tenths of;
#X text 232 191 fundamental);
#X text 29 259 frequency;
#X obj 227 427 cos~;
#X obj 268 340 wrap~;
#X obj 232 367 -~;
#X obj 227 397 +~;
#X obj 232 464 -~;
#X obj 247 494 *~;
#X obj 225 519 +~;
#X obj 59 578 tabwrite~ carrier;
#X obj 33 308 phasor~ 40;
#X obj 232 289 pack 0 50;
#X text 27 36 The other \, spiffier way is to make a sum of cosines
to interpolate between adjacent harmonics. Suppose for example we want
a center frequency of 5.3 (in units of the fundamental.) We just take
partial 5 with amplitude 0.7 and partial 6 with amplitude 0.7:;
#X text 451 581 updated for Pd version 0.34;
#X text 281 366 subtract to get the integer part "n";
#X text 277 399 multiply phase by n and n+1;
#X text 282 427 synthesize the two partials;
#X text 54 526 graph;
#X text 347 548 <--output;
#X text 323 339 the fractional part "b";
#X text 280 463 p2 - p1;
#X text 295 492 b * (p2 - p1);
#X text 264 519 b * p2 + (1-b) * p1;
#X connect 0 0 1 1;
#X connect 1 0 0 0;
#X connect 2 0 1 2;
#X connect 3 0 27 0;
#X connect 4 0 24 1;
#X connect 4 0 26 0;
#X connect 5 0 6 0;
#X connect 6 0 11 0;
#X connect 8 0 4 0;
#X connect 8 0 23 0;
#X connect 10 0 22 0;
#X connect 10 0 21 0;
#X connect 11 0 29 0;
#X connect 13 0 28 0;
#X connect 20 0 24 0;
#X connect 21 0 22 1;
#X connect 21 0 25 1;
#X connect 22 0 8 1;
#X connect 23 0 20 0;
#X connect 24 0 25 0;
#X connect 25 0 26 1;
#X connect 26 0 1 0;
#X connect 26 0 27 0;
#X connect 28 0 8 0;
#X connect 28 0 23 1;
#X connect 29 0 10 0;
