## FujiFilm Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | Version | undef |
> 0x0010 | InternalSerialNumber | string | (this number is unique, and contains the date of manufacture, but doesn't necessarily correspond to the camera body number -- this needs to be checked)
> 0x1000 | Quality | string |
> 0x1001 | Sharpness | int16u | 1 = Soft 2 = Soft2 3 = Normal 4 = Hard 5 = Hard2
> 0x1002 | WhiteBalance | int16u | 0x0 = Auto 0x100 = Daylight 0x200 = Cloudy 0x300 = Daylight Fluorescent 0x301 = Day White Fluorescent 0x302 = White Fluorescent 0x400 = Incandescent 0x500 = Flash 0xf00 = Custom 0xff0 = Kelvin
> 0x1003 | Saturation | int16u | 0x0 = Normal 0x100 = High 0x200 = Low 0x300 = None (B&W)
> 0x1004 | Contrast | int16u | 0x0 = Normal 0x100 = High 0x200 = Low
> 0x1005 | ColorTemperature | int16u |
> 0x1010 | FujiFlashMode | int16u | 0 = Auto 1 = On 2 = Off 3 = Red-eye reduction
> 0x1011 | FlashStrength | rational64s |
> 0x1020 | Macro | int16u | 0 = Off 1 = On
> 0x1021 | FocusMode | int16u | 0 = Auto 1 = Manual
> 0x1023 | FocusPixel | int16u[2] |
> 0x1030 | SlowSync | int16u | 0 = Off 1 = On
> 0x1031 | PictureMode | int16u | 0x0 = Auto 0x1 = Portrait 0x2 = Landscape 0x4 = Sports 0x5 = Night Scene 0x6 = Program AE 0x7 = Natural Light 0x8 = Anti-blur 0xa = Sunset 0xb = Museum 0xc = Party 0xd = Flower 0xe = Text 0xf = Natural Light & Flash 0x10 = Beach 0x11 = Snow 0x12 = Fireworks 0x13 = Underwater 0x100 = Aperture-priority AE 0x200 = Shutter speed priority AE 0x300 = Manual
> 0x1100 | AutoBracketing | int16u | 0 = Off 1 = On 2 = No flash & flash
> 0x1101 | SequenceNumber | int16u |
> 0x1210 | ColorMode | int16u | 0x0 = Standard 0x10 = Chrome 0x30 = B & W
> 0x1300 | BlurWarning | int16u | 0 = None 1 = Blur Warning
> 0x1301 | FocusWarning | int16u | 0 = Good 1 = Out of focus
> 0x1302 | ExposureWarning | int16u | 0 = Good 1 = Bad exposure
> 0x1400 | DynamicRange | int16u | 1 = Standard 3 = Wide
> 0x1401 | FilmMode | int16u | 0x0 = F0/Standard 0x100 = F1/Studio Portrait 0x200 = F2/Fujichrome 0x300 = F3/Studio Portrait Ex 0x400 = F4/Velvia
> 0x1402 | DynamicRangeSetting | int16u | 0x0 = Auto (100-400%) 0x1 = RAW 0x100 = Standard (100%) 0x200 = Wide1 (230%) 0x201 = Wide2 (400%) 0x8000 = Film Simulation Mode
> 0x1403 | DevelopmentDynamicRange | int16u |
> 0x1404 | MinFocalLength | rational64s |
> 0x1405 | MaxFocalLength | rational64s |
> 0x1406 | MaxApertureAtMinFocal | rational64s |
> 0x1407 | MaxApertureAtMaxFocal | rational64s |
> 0x8000 | FileSource | string |
> 0x8002 | OrderNumber | int32u |
> 0x8003 | FrameNumber | int16u |

## FujiFilm RAF Tags

Tags extracted from FujiFilm RAF-format information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0100 | RawImageFullSize | N | (including borders)
> 0x0121 | RawImageSize | N |
> 0x0130 | FujiLayout | N |
> 0x2ff0 | WB_GRGBLevels | N |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Oct 15, 2007

<-- ExifTool Tag Names